Linux nForce Driver - AMD64/EM64T

 
Version: 1.0-0310
Release Date: November 23, 2005

Release Highlights for 1.0-0310:

Adds support for nForce 430/410 motherboards 
Adds support for 8-bit audio playback 
Compatibility fixes 
This page contains drivers and documentation for the nForce chipset. The chipset includes hardware support for IDE disk control, Ethernet networking, audio support, win modem support, and a USB controller. These packages have support for Ethernet networking and basic ACI audio. USB and IDE hardware will work with standard Linux drivers. There is no win modem support.


To download and install the drivers, follow the steps below:


STEP 1: Download the Driver File
Download - NFORCE-Linux-x86_64-1.0-0310-pkg1.run
         - NFORCE-Linux-x86_32-1.0-0310-pkg1.run

STEP 2: Begin Installation
From within a shell with root privileges, type "sh NFORCE-Linux-x86_64-1.0-0310-pkg1.run" to initiate the installation.

STEP 3: Review the NVIDIA Software License. You will need to accept this license to continue with the installation.

STEP 4: Review the Known Problems for any special installation instructions required by your platform.


STEP 5: Install
Follow the directions provided by the installer.  The installer will prepare the driver and install the driver and application files in the appropriate place.


Note:  For systems running a kernel for which there is no pre-built binary driver, the installer will need to build the driver.  In order for the installer to build the driver, the kernel source needs to be installed.


STEP 6: Review Documentation
Refer to the ReleaseNotes (HTML Version) file (installed in /usr/share/doc/nforce) for instructions on configuring the system with the installed drivers.


If you have any questions or problems, please check the linux discussion forum. If you don't find an answer to your question there, you can send email to linux-nforce-bugs@nvidia.com



Copyright c 2005 NVIDIA Corporation
Legal Info | Privacy Policy | Subscribe to the NVIDIA Newsletter 
 
