;


















; Remote Control HID Minidriver Installation


















; for the 64-bit Windows


















;


















; Copyright (c) 2000-2006 Widcomm/Broadcom


















;


















[version]


















signature="$Windows NT$"


















Class=HIDClass


















ClassGUID={745a17a0-74d3-11d0-b6fe-00a0c90f57da}


















Provider=%V_WIDCOMM%


















CatalogFile=btwrchid64.cat


















DriverVer=03/11/2008,6.1.0.4500





































[DestinationDirs]


















CopyFiles.amd64 = 12





































[SourceDisksNames]


















1 = %Source_Description%,,,





































[SourceDisksFiles]


















btwrchid.sys = 1


















btwavdt.sys = 1





































[Manufacturer] 


















%V_WIDCOMM%=WIDCOMM, NTamd64





































[WIDCOMM.NTamd64]


















; BTW id


















%WC_AVCONTROL_DESCRIPTION%=WC_AVCONTROL, {95C7A0A0-3094-11D7-A202-00508B9D7D5A}\HIDAVCONTROL


















; MSFT id


















%WC_AVCONTROL_DESCRIPTION%=WC_AVCONTROL,BTHENUM\{84A1E9B8-12BA-4a9c-8AB0-A43784E0D149}





































[WC_AVCONTROL.NTamd64.hw]


















AddReg=WC_AVCONTROL.hw.reg





































[WC_AVCONTROL.hw.reg]


















HKR,,"Usage",0x10001,%HID_USAGE_GENERIC_AVCONTROL%


















HKR, ,LowerFilters, 0x00010000, "btwavdt"





































[WC_AVCONTROL.NTamd64]


















CopyFiles = CopyFiles.amd64





































[WC_AVCONTROL.NTamd64.Services]


















AddService = btwrchid,0x00000002,BTWRCHID_Serv_Inst,


















AddService=btwavdt,,btwavdt_Service_Inst





































[BTWRCHID_Serv_Inst] 


















ServiceType = %SERVICE_KERNEL_DRIVER% 


















StartType = %SERVICE_DEMAND_START% 


















ErrorControl = %SERVICE_ERROR_IGNORE% 


















ServiceBinary = %12%\btwrchid.sys 





































[btwavdt_Service_Inst]


















DisplayName = %btwavdt.SvcDesc%


















ServiceType = %SERVICE_KERNEL_DRIVER% 


















StartType = %SERVICE_DEMAND_START% 


















ErrorControl = %SERVICE_ERROR_IGNORE% 


















ServiceBinary = %12%\btwavdt.sys





































[CopyFiles.amd64] 


















btwrchid.sys


















btwavdt.sys





































[Strings] 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM Installation Media"


















V_WIDCOMM="Broadcom"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"


















btwavdt.SvcDesc="Bluetooth AVDT"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20
























































[Strings.0404] ; Chinese Traditional 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM 安裝媒體"


















V_WIDCOMM="Broadcom"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"


















btwavdt.SvcDesc="Bluetooth AVDT"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0406] ; Danish 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-installationsmedie"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0407] ; German 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-Installationsmedien"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.040a] ; Spanish


















;  *******Localizable Strings******* 


















Source_Description="Medios de instalación de WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.040b] ; Finnish 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-asennuslevy"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.040c] ; French 


















;  *******Localizable Strings******* 


















Source_Description="Support d'installation WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0410] ; Italian 


















;  *******Localizable Strings******* 


















Source_Description="Supporto di installazione WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0411] ; Japanese 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM インストール メディア"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0412] ; Korean 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM 설치 미디어"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0413] ; Dutch 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-installatiemedia"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0416] ; Brazilian Portuguese 


















;  *******Localizable Strings******* 


















Source_Description="Mídia de instalação WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_MOUSE = 0x80


















HID_USAGE_GENERIC_KEYBOARD = 0x40


















HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.041d] ; Swedish 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-installationsskiva"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0415] ; Polish 


















;  *******Localizable Strings******* 


















Source_Description="Noœnik instalacyjny WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0419] ; Russian 


















;  *******Localizable Strings******* 


















Source_Description="Носитель для установки WIDCOMM"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0414] ; Norwegian 


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM-installasjonsmedier"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20





































[Strings.0804] ; ChineseSimplified


















;  *******Localizable Strings******* 


















Source_Description="WIDCOMM 安装介质"


















V_WIDCOMM="Broadcom"


















btwavdt.SvcDesc="Bluetooth AVDT"


















WC_AVCONTROL_DESCRIPTION= "Bluetooth Remote Control"





































;  *******Non Localizable Strings******* 


















SERVICE_BOOT_START = 0x0 


















SERVICE_SYSTEM_START = 0x1 


















SERVICE_AUTO_START = 0x2 


















SERVICE_DEMAND_START = 0x3 


















SERVICE_DISABLED = 0x4 





































SERVICE_KERNEL_DRIVER = 0x1 


















SERVICE_ERROR_IGNORE = 0x0 


















SERVICE_ERROR_NORMAL = 0x1 


















SERVICE_ERROR_SEVERE = 0x2 


















SERVICE_ERROR_CRITICAL = 0x3 





































HID_USAGE_GENERIC_AVCONTROL = 0x20


















