--------------------------------------------------------------------------------
           VIA RAID RHEL 4.0 Software Release History
                    Release Package Version: 2.10
                    Release Date: 03/31/2006
                    
                    Linux Driver Version:   2.10
                    
                    Linux RaidTool Version: 2.10
                    
--------------------------------------------------------------------------------

1. Features

   Hardware                 VIA RAID Controller(VT6410, VT6420/8237, VT6421, VT8251)
   Transfer Rate            PIO Mode
                            DMA Mode

   RAID Level               RAID0, RAID1, RAID0+1, JBOD, RAID5, None RAID
   Support Device           ATA/SATA/SATA2 Device. up to four hard disk drives totally
                              
   Operating System         RHEL 4.0 AS 
   			    RHEL 4.0 WS
			    RHEL 4.0 Desktop

2. Notes
    Please enter the following command while you install OS .
    #linux dd acpi=off 
    or 
    #linux dd pci=conf1
    And then add the same command on bootloader option after installing OS . 
   

3. Limitations  
  a. Can't use VIA Linux V-RAID Tool V2.10 for VT8251 RAID Mode 5 Migration testing. 
  b. Can't use VIA Linux V-RAID Tool V2.10 for RAID Mode 0 Migration testing .
  
